**NETFW001**

LAN

|  |  |  |  |
| --- | --- | --- | --- |
| **Source** | **Destination** | **Port** | **Action** |
| Admin-PC | SRVWS001 | 22 | Accept |
| Admin-PC | SRVFT001 | 22 | Accept |
| Admin-PC | AP-WLAN | 443 | Accept |
| Clients-LAN | SRVWS001 | 443 | Accept |
| Clients-LAN | SRVFT001 | 445 | Accept |
| Clients-LAN | WAN | 465 | Accept |
| Clients-LAN | WAN | Surfen | Accept |
| VPN-NET | SRVFS001 | 445 | Accept |
| ALL | ALL | ALL | Drop |

DMZ

|  |  |  |  |
| --- | --- | --- | --- |
| **Source** | **Destination** | **Port** | **Action** |
| SRVWS001 | SRVDB001 | 3306 | Accept |
| ALL | ALL | ALL | Drop |
|  |  |  |  |
|  |  |  |  |

WAN

|  |  |  |  |
| --- | --- | --- | --- |
| **Source** | **Destination** | **Port** | **Action** |
| ANY | WAN | VPN-Group | ENCRYPT |
| WAN | SRVWS001 | 443 | Accept |
| WAN | SRVFT001 | 445 | Accept |
| ALL | ALL | ALL | Drop |
|  |  |  |  |

WLAN

|  |  |  |  |
| --- | --- | --- | --- |
| **Source** | **Destination** | **Port** | **Action** |
| AP-WLAN | WAN | ALL | Accept |
| WLAN-Clients | WAN | ALL | Accept |
| ALL | ALL | ALL | Drop |

(Letzte Regel dient nur der Vollständigkeit, nicht zwingend nötig.)